Design and Access statement

Original Farmhouse Built C16 with several extensions over the last 500yrs with the latest extension built C20, which has been de-listed.

The property construction is with brick walls with white painted render under a tiled roof.
The existing windows are white painted timber flush casements with astragal bar, which are C21.

The proposal is to replace existing windows with Residence 9 flush casements which are white woodgrain composite (PVCu) with astragal bar. Ironmongery to be butt hinges, monkey tail handles and traditional peg stay all to match existing.

I anticipate that there will be no visual change in appearance to the property. 
[bookmark: _GoBack]The change to the property would be a much greater thermal efficiency helping to lower our carbon footprint. It will also retain its appearance and listed building status which we would not want to detract from.

There would be no change to the design or access to the property.

